TN70E-B8026 Firmware Release Note

;****************************************************************************
;****************************************************************************
;**             (C)Copyright 1987-2020, TYAN COMPUTER CORP.                **
;**                                                                        **
;**                      http://www.tyan.com                               **
;**                                                                        **
;**                                                                        **
;****************************************************************************
;****************************************************************************
------------------------------<< LOG >>-------------------------------
v4.00	- Date     : 03/24/2020
			- Filename: 80263204.ima
			- Checksum: 9336<H>
			- Description
			  - Based on  80263202.ima
			  - Force password change for fixed user at first login
			  - Disable DIMM sensor scan when BIOS post to support NVDIMM(Please co-work with support NVME DIMM BIOS)
			  - Enable host interface(Support BIOS communicate with BMC via redfish)
			  - Preserve uploaded SSL certificate info during BMC FW update
			  - Update gTLD validation rule
			  - Add PSU FRU(PSU0/PSU1)
                          - Add set t_high oem command
			  - Modify temperature sensor Entity ID/Instance
			  - Update Set PCIE info command
			  - Disable RTC_VBAT upper threshold
*Note 1: Due to image layout is modified, please use socflash utility to update the BMC FW.
*Note 2: Please follow the update process to update BMC FW first then program the new BIOS with Redfish enabled.
================================================================================	

	   